**Name of Work:- Construction of Parking Shade and Service Deck**

**BOQ**

Rate Based on MRS-20

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **A: - Construction of Parking Shade** | | | | | | |
| **S.No** | **Item Code** | **Description** | **Unit** | **Qty** | **Rate** | **Amount** |
| 1 | 03.51 | Excavation of Trench In all kind of soil | 1000 ft | 0.756 | 5218.50 | 3,945 |
| 2 | 06-05-i | p.c.c 1:18 | 100 ft | 31.50 | 17001.94 | 535,561 |
| 3 | 06-05-f | P.c.c 1:2:4 | 100 ft | 15.83 | 22039.19 | 348,880 |
| 4 | 14-98-a | S/F M.s Pipe 4” i/d 5mm Thick | RFT | 504 | 1264.02 | 637,066 |
| 5 | 09-14-b | S/F Corrugated G.I sheet with G.I bolt,nuts,limpet, etc complete | 100 sft | 40.32 | 19552.38 | 788,352 |
|  |  |  |  | Total | Rs | 2,313,804 |
| **B:- Service Deck** | | | | | | |
| 6 | 03.51 | Excavation for Trench in all kind of soil | 1000 ft | 0.600 | 5218.5 | 3,131 |
| 7 | 06-05-i | p.c.c 1:18 | 100 ft | 6.00 | 17001.94 | 102,012 |
| 8 | 06-05-f | P.c.c 1:2:4 | 100ft | 3.00 | 22039.19 |  |
| 9 | 07-05-a-02 | B.B masnory in 1:3 csm | 100 ft | 2.5992 | 28748.83 | 74,724 |
| 10 | 11-04-a | Cement plaster 1:2 | 100 sft | 7.20 | 2789.96 | 20,087 |
|  |  |  |  | Total | Rs | 266,072 |
|  |  | **Total A+B** |  |  | **Rs** | **2,579,876** |

Contractor above, below at par\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Deputy Director (Civil)